Seatbelts with contact sensors and speed switch.

A Microcontroller (Arduino) detects the condition of seatbelt and speed.

It then gives data to a RF Transmitter which transmits this information.

The processed information is received by the receiver unit.

The receiver unit transfers this information to the PC for further processing.

After processing the computer displays the final results on the screen.